Problem 2:

# 4- BER is a decaying curve; because as E/N0 increases the signal to noise ratio increase, meaning that the signal power is much larger that noise. So the bit rate error decreases.

5- From the plotted graphs, the third matched filter (MF = sqrt(3)) has the best BER, it reaches ‘0’ faster than the other two cases, nearly at SNR = 0